

## **FAMCO SERVICE & MACHINE DELIVERS TECHNICAL EXPERTISE & SOLUTIONS THAT**

Structural Inspection Report

**Account:** {{Account}}

**Address:**

{{Street}}

{{City}}

{{State}}

{{PostalCode}}

**Phone:** {{AccountPhone}}

**Asset Inspected:** {{AssetName}}

***Inspection ID: {{InspectionID}}***

**Please provide pictures of the general condition of the machine in its current state.**

1. **Welds:**

All welds are acceptable and free of cracks. ***{{Welds}}***

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Foundation / Anchors:** (*If applicable*)

Foundation was acceptable. Machine does not move during operation and all anchors are tight and secured as required. ***{{Foundation}}***

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Cylinder Mount:**

Cylinder mount pins and retainers are intact and secure. Cylinder mount block welds are intact and free from cracks and damage. ***{{CylinderMounts}}***

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Knives:**

Were the Knives inspected? ***{{Knives}}***

The initial inspection reveals the Knives are ***{{KnivesOutcome}}.***

During the inspection the knife gap was found to be at ***{{KnifeGap}}.***

OEM knife gap requirements for this piece of equipment, should be set at ***{{OEMKnifeGap}}***, per operator’s manual.

To meet the OEM requirements the Knife Gap was adjusted to: ***{{KnivesAdjustedTo}}***

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Liners:**

All machine liners have been inspected and thicknesses have been documented. ***{{Liners}}***

Liners have been inspected for broken or missing bolts. ***{{LinerBolts}}***

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Hold Downs:**

Hold down liners have been checked and adjusted as needed. ***{{HoldDowns}}***